{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Main","Rs-Origin","RS-New","Grafico","DP+WB"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Grafico","index":3,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":false,"merged":[[0,1,0,2],[7,1,7,2],[11,1,11,2]]}
[null,"Instructions"]
[null,"Save the RS internet page (http://weather.uwyo.edu/upperair/sounding.html) in txt format in your computer in a disc and folder your prefer","ATTENTION: do not copy the RS in a text file and save it! Do not use  Include frost point calculations AND Recalculate Data"]
[null,"Eventually rename the RS as you like, example \"20160101 00z Linate.txt\""]
[null,"Configure this program (see config below)"]
[null,"Click the button to activate the program"]
[null,"Click on the right link to see the result","RS-New'!A1"]
[]
[null,"Config"]
[null,"DRIVE with RS","S:"]
[null,"FOLDER with RS (NO slash at the end)","\\Radiosondaggi"]
[]
[null,"Graph"]
[]
[null,"Max Graph Height [metri]",2000]
[null,"Temperatura Min Grafico [gradi]",-15]
[null,"Reset Graph to Autoscale"]

{"sheet":"Rs-Origin","index":1,"n_rows":143,"n_cols":12,"rows_kept":143,"cut":false,"hidden":false,"merged":[]}
[]
[null,10868,"Muenchen-Oberschlssheim","Observations","at","12Z",3,"Jan",2016]
[]
["-----------------------------------------------------------------------------"]
[null,"PRES","HGHT","TEMP","DWPT","RELH","MIXR","DRCT","SKNT","THTA","THTE","THTV"]
[null,"hPa","m","C","C","%","g/kg","deg","knot","K","K","K"]
["-----------------------------------------------------------------------------"]
[null,1000,100]
[null,953,492,0.2,-1.6,88,3.58,55,2,277.10000000000002,287.2,277.7]
[null,936,635,-2.2000000000000002,-2.6,97,3.38,335,2,276.2,285.60000000000002,276.7]
[null,935,643,-2.2999999999999998,-2.7,97,3.37,328,3,276.10000000000002,285.5,276.7]
[null,928,703,1.4,1,97,4.45,277,8,280.5,293,281.2]
[null,925,729,1.4,1,97,4.47,255,10,280.7,293.3,281.5]
[null,923,746,1.5,1.1000000000000001,97,4.5,255,10,281,293.7,281.8]
[null,920,773,1.6,1.2,97,4.5599999999999996,258,11,281.39999999999998,294.2,282.10000000000002]
[null,905,904,0.9,0.5,97,4.42,275,16,282,294.5,282.8]
[null,889,1047,0.2,-0.2,97,4.26,290,14,282.7,294.8,283.39999999999998]
[null,861,1304,-1.2,-1.5,98,4,255,8,283.89999999999998,295.39999999999998,284.60000000000002]
[null,850,1407,-1.7,-2,98,3.9,260,10,284.39999999999998,295.60000000000002,285]
[null,839,1509,-2.4,-2.7,98,3.75,255,10,284.7,295.5,285.3]
[null,793,1950,-5.3,-5.7,97,3.16,295,12,286.2,295.39999999999998,286.7]
[null,759,2293,-7.6,-8.1,97,2.76,290,14,287.3,295.5,287.8]
[null,745,2439,-8.6,-9.1,97,2.6,305,12,287.8,295.5,288.2]
[null,713,2783,-10.9,-11.4,96,2.25,273,10,288.89999999999998,295.7,289.3]
[null,710,2815,-11.1,-12.5,89,2.0699999999999998,270,10,289,295.2,289.3]
[null,700,2924,-11.9,-16.3,70,1.54,305,4,289.3,294,289.60000000000002]
[null,698,2946,-11.9,-18.899999999999999,56,1.24,304,4,289.5,293.39999999999998,289.7]
[null,663,3339,-12.9,-15,84,1.81,295,3,292.7,298.3,293]
[null,632,3704,-14.3,-18.3,72,1.44,285,2,295.10000000000002,299.7,295.39999999999998]
[null,628,3752,-13.9,-18.399999999999999,69,1.44,284,2,296.10000000000002,300.7,296.39999999999998]
[null,615,3910,-14.8,-19.600000000000001,67,1.33,280,2,296.89999999999998,301.2,297.10000000000002]
[null,565,4549,-18.3,-24.3,59,0.95,250,8,300,303.2,300.2]
[null,549,4761,-20,-25.5,61,0.88,240,10,300.5,303.39999999999998,300.60000000000002]
[null,500,5450,-25.5,-29.5,69,0.67,315,6,301.89999999999998,304.2,302]
[null,432,6495,-33.700000000000003,-40.700000000000003,49,0.25,246,5,304.3,305.3,304.39999999999998]
[null,419,6708,-35.700000000000003,-41.7,54,0.24,232,4,304.39999999999998,305.3,304.5]
[null,412,6826,-36.5,-46.5,35,0.14000000000000001,224,4,304.89999999999998,305.39999999999998,304.89999999999998]
[null,400,7030,-38.5,-46.5,43,0.15,210,4,304.89999999999998,305.39999999999998,304.89999999999998]
[null,390,7203,-40.1,-47.1,47,0.14000000000000001,198,4,305,305.5,305]
[null,383,7326,-41.1,-51.1,33,0.09,190,4,305.3,305.60000000000002,305.3]
[null,376,7451,-42.1,-55.1,23,0.06,208,5,305.60000000000002,305.8,305.60000000000002]
[null,356,7814,-45.1,-57.3,24,0.05,260,10,306.3,306.5,306.3]
[null,339,8140,-47.8,-59.2,26,0.04,265,21,306.89999999999998,307.10000000000002,306.89999999999998]
[null,330,8319,-49.3,-60.3,26,0.03,295,27,307.3,307.39999999999998,307.3]
[null,327,8378,-49.4,-62.5,20,0.03,305,29,307.89999999999998,308,307.89999999999998]
[null,311,8706,-50.1,-74.2,4,0.01,320,43,311.39999999999998,311.39999999999998,311.39999999999998]
[null,307,8790,-50.3,-77.3,3,0,318,43,312.3,312.3,312.3]
[null,300,8940,-51.3,-70.3,9,0.01,315,43,312.89999999999998,313,312.89999999999998]
[null,286,9250,-53.3,-68.3,14,0.01,318,49,314.39999999999998,314.39999999999998,314.39999999999998]
[null,280,9386,-53.9,-77.900000000000006,4,0,319,51,315.39999999999998,315.39999999999998,315.39999999999998]
[null,277,9455,-54.2,-77.5,4,0,320,52,316,316,316]
[null,253,10034,-56.5,-74.5,9,0.01,315,43,320.89999999999998,320.89999999999998,320.89999999999998]
[null,250,10110,-55.9,-76.900000000000006,6,0,315,47,322.8,322.89999999999998,322.8]
[null,237,10450,-55.4,-80.5,3,0,330,45,328.5,328.5,328.5]
[null,224,10809,-55,-84.4,1,0,310,43,334.6,334.6,334.6]
[null,203,11435,-54.1,-91.1,0,0,310,41,345.5,345.5,345.5]
[null,200,11530,-54.1,-91.1,0,0,310,41,346.9,346.9,346.9]
[null,183,12098,-54.5,-91.2,0,0,310,33,355.1,355.1,355.1]
[null,153,13243,-55.4,-91.5,0,0,310,37,372.3,372.3,372.3]
[null,150,13370,-55.5,-91.5,0,0,305,43,374.2,374.2,374.2]
[null,144,13629,-55.6,-91.6,0,0,295,43,378.5,378.5,378.5]
[null,132,14180,-55.8,-91.8,0,0,295,45,387.7,387.7,387.7]
[null,119,14837,-56,-92,0,0,300,39,399,399,399]
[null,114,15109,-56,-92,0,0,285,43,403.8,403.8,403.8]
[null,100,15940,-56.3,-92.3,0,0,300,37,418.7,418.7,418.7]
[null,90.7,16563,-54.9,-90.9,0,0,290,41,433.3,433.3,433.3]
[null,86,16901,-55.6,-91.3,0,0,285,43,438.6,438.6,438.6]
[null,77,17604,-56.9,-92.3,0,0,310,33,449.8,449.9,449.8]
[null,72,18031,-57.8,-92.9,0,0,310,21,456.8,456.8,456.8]
[null,70,18210,-58.1,-93.1,0,0,290,19,459.7,459.8,459.7]
[null,68,18393,-58.1,-93.1,0,0,270,25,463.6,463.6,463.6]
[null,62,18975,-58,-93,0,0,285,49,476.1,476.1,476.1]
[null,54,19845,-58,-93,0,0,275,31,495.5,495.5,495.5]
[null,51,20205,-57.9,-92.9,0,0,260,35,503.7,503.7,503.7]
[null,50,20330,-57.9,-92.9,0,0,260,33,506.6,506.6,506.6]
[null,48,20587,-58.2,-93.2,0,0,275,41,511.9,511.9,511.9]
[null,44.1,21120,-58.7,-93.7,0,0,275,50,523.1,523.20000000000005,523.1]
[null,44,21134,-58.7,-93.7,0,0,275,51,523.4,523.4,523.4]
[null,39,21883,-61,-95.5,0,0,265,37,535.9,536,535.9]
[null,37,22210,-62,-96.3,0,0,260,39,541.5,541.5,541.5]
[null,35,22555,-63.1,-97.1,0,0,273,41,547.4,547.4,547.4]
[null,34,22735,-62.5,-96.7,0,0,280,43,553.5,553.5,553.5]
[null,30,23510,-59.9,-94.9,0,0,280,52,580.79999999999995,580.79999999999995,580.79999999999995]
[null,27,24171,-58.1,-93.1,0,0,280,58,603.5,603.5,603.5]
[null,26.3,24336,-57.7,-92.7,0,0,278,54,609.20000000000005,609.29999999999995,609.20000000000005]
[null,25,24654,-58.4,-93.2,0,0,275,47,616.20000000000005,616.20000000000005,616.20000000000005]
[null,21,25745,-60.7,-94.8,0,0,270,54,640.79999999999995,640.79999999999995,640.79999999999995]
[null,20,26050,-61.3,-95.3,0,0,270,56,647.79999999999995,647.79999999999995,647.79999999999995]
[null,19.7,26144,-61.5,-95.5,0,0,269,59,650,650,650]
[null,18,26709,-60.1,-94.8,0,0,265,76,671.5,671.5,671.5]
[null,17,27067,-59.2,-94.3,0,0,275,85,685.4,685.5,685.4]
[null,16,27446,-58.2,-93.8,0,0,270,80,700.5,700.6,700.5]
[null,15.1,27809,-57.3,-93.3,0,0,271,85,715.2,715.3,715.2]
[null,13.3,28608,-59.1,-94.1,0,0,272,97,735.5,735.5,735.5]
[null,10,30440,-48.7,-86.7,0,0.02,275,124,836.7,836.9,836.7]
[null,9,31149,-45.2,-84.5,0,0.04,270,109,875.8,876.3,875.8]
[null,7.2,32651,-37.700000000000003,-79.7,0,0.1,283,143,964,965.4,964.1]
[null,6.6,33247,-40.5,-81.5,0,0.08,288,156,976.5,977.7,976.6]
[null,6.4,33459,-39.4,-80.900000000000006,0,0.09,290,161,989.8,991.1,989.9]
[null,6,33903,-37.1,-79.599999999999994,0,0.12,290,161,1018.1,1020,1018.2]
[null,5.8,34136,-35.9,-78.900000000000006,0,0.14000000000000001,1033.3,1035.4000000000001,1033.4000000000001]
[]
[]
[null,"Station","information","and","sounding","indices"]
[]
[null,"Station","number:",10868]
[null,"Observation","time:","160103/1200"]
[null,"Station","latitude:",48.25]
[null,"Station","longitude:",11.55]
[null,"Station","elevation:",492]
[null,"Showalter","index:",6.61]
[null,"Lifted","index:",9.92]
[null,"LIFT","computed","using","virtual","temperature:",9.9700000000000006]
[null,"SWEAT","index:",25.25]
[null,"K","index:",17.399999999999999]
[null,"Cross","totals","index:",23.5]
[null,"Vertical","totals","index:",23.8]
[null,"Totals","totals","index:",47.3]
[null,"Convective","Available","Potential","Energy:",0]
[null,"CAPE","using","virtual","temperature:",0]
[null,"Convective","Inhibition:",0]
[null,"CINS","using","virtual","temperature:",0]
[null,"Bulk","Richardson","Number:",0]
[null,"Bulk","Richardson","Number","using","CAPV:",0]
[null,"Temp","[K]","of","the","Lifted","Condensation","Level:",272.67]
["Pres","[hPa]","of","the","Lifted","Condensation","Level:",915.34]
[null,"Mean","mixed","layer","potential","temperature:",279.67]
[null,"Mean","mixed","layer","mixing","ratio:",4.08]
[null,1000,"hPa","to",500,"hPa","thickness:",5350]
["Precipitable","water","[mm]","for","entire","sounding:",11.7]
[]
["Description","of","the","data","columns"]
["<http://weather.uwyo.edu/upperair/columns.html>","or","sounding","indices"]
["<http://weather.uwyo.edu/upperair/indices.html>."]
[]
["------------------------------------------------------------------------"]
["/Interested","in","graduate","studies","in","atmospheric","science?","Check","out","our"]
["program","at","the","University","of","Wyoming"]
["<http://www.uwyo.edu/atsc/howtoapply/>/"]
["------------------------------------------------------------------------"]
["Questions","about","the","weather","data","provided","by","this","site","can","be","addressed"]
["to","Larry","Oolman","(ldoolman@uwyo.edu)","<mailto:ldoolman@uwyo.edu>"]
["------------------------------------------------------------------------"]

{"sheet":"RS-New","index":2,"n_rows":44,"n_cols":13,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
[10868,"Muenchen-Oberschlssheim",null,3,"Jan",2016,null,null,"Go back to Main Sheet",null,null,"Main!A1"]
["PRES","HGHT","TEMP","DWPT","RELH","MIXR","DRCT","SKNT","THTA","THTE","THTV","DP","WB"]
["hPa","m","C","C","%","g/kg","deg","knot","K","K","K","°C","°C"]
[953,492,0.2,-1.6,88,3.58,55,2,277.10000000000002,287.2,277.7,-1.5495298873221539,-0.48365128040313721]
[936,635,-2.2000000000000002,-2.6,97,3.38,335,2,276.2,285.60000000000002,276.7,-2.6108053068154349,-2.3538920879364014]
[935,643,-2.2999999999999998,-2.7,97,3.37,328,3,276.10000000000002,285.5,276.7,-2.7104568056796743,-2.4533343315124512]
[928,703,1.4,1,97,4.45,277,8,280.5,293,281.2,0.97655033482552589,1.2216947078704834]
[925,729,1.4,1,97,4.47,255,10,280.7,293.3,281.5,0.97655033482552589,1.2214347124099731]
[923,746,1.5,1.1000000000000001,97,4.5,255,10,281,293.7,281.8,1.0761963716848741,1.3205841779708862]
[920,773,1.6,1.2,97,4.5599999999999996,258,11,281.39999999999998,294.2,282.10000000000002,1.1758422609287025,1.4196455478668213]
[905,904,0.9,0.5,97,4.42,275,16,282,294.5,282.8,0.47831793628447938,0.72307878732681274]
[889,1047,0.2,-0.2,97,4.26,290,14,282.7,294.8,283.39999999999998,-0.21921362161672386,2.6395255699753761E-2]
[{"$f":"(A14-A12)/($M14-$M12)*($M13-$M12)+A12","v":888.4473598904118},{"$f":"(B14-B12)/($M14-$M12)*($M13-$M12)+B12","v":1052.0724467201483},0.17236799452059282,-0.2256582908023067,97.019737146771007,4.2548683418395381,289.30919986301484,13.881577119373969,282.72368457612521,294.81184228806262,283.4236845761252,-0.24399835980564732,0]
[861,1304,-1.2,-1.5,98,4,255,8,283.89999999999998,295.39999999999998,284.60000000000002,-1.474954305743037,-1.3109437227249146]
[850,1407,-1.7,-2,98,3.9,260,10,284.39999999999998,295.60000000000002,285,-1.9737936101807156,-1.8093854188919067]
[839,1509,-2.4,-2.7,98,3.75,255,10,284.7,295.5,285.3,-2.6721727561423299,-2.5069756507873535]
[793,1950,-5.3,-5.7,97,3.16,295,12,286.2,295.39999999999998,286.7,-5.7000704200952601,-5.4461383819580078]
[759,2293,-7.6,-8.1,97,2.76,290,14,287.3,295.5,287.8,-7.9921975092705297,-7.7347583770751953]
[745,2439,-8.6,-9.1,97,2.6,305,12,287.8,295.5,288.2,-8.9887988658163742,-8.7298622131347656]
[713,2783,-10.9,-11.4,96,2.25,273,10,288.89999999999998,295.7,289.3,-11.410382488210413,-11.05870532989502]
[710,2815,-11.1,-12.5,89,2.0699999999999998,270,10,289,295.2,289.3,-12.54837435877257,-11.537638664245605]
[700,2924,-11.9,-16.3,70,1.54,305,4,289.3,294,289.60000000000002,-16.244863758014713,-13.087216377258301]
[698,2946,-11.9,-18.899999999999999,56,1.24,304,4,289.5,293.39999999999998,289.7,-18.879088274322676,-13.678832054138184]
[663,3339,-12.9,-15,84,1.81,295,3,292.7,298.3,293,-15.026130016815735,-13.504734039306641]
[632,3704,-14.3,-18.3,72,1.44,285,2,295.10000000000002,299.7,295.39999999999998,-18.223785398360185,-15.321974754333496]
[628,3752,-13.9,-18.399999999999999,69,1.44,284,2,296.10000000000002,300.7,296.39999999999998,-18.337764589970373,-15.064974784851074]
[615,3910,-14.8,-19.600000000000001,67,1.33,280,2,296.89999999999998,301.2,297.10000000000002,-19.544049282376069,-15.995011329650879]
[565,4549,-18.3,-24.3,59,0.95,250,8,300,303.2,300.2,-24.317566398597627,-19.564624786376953]
[549,4761,-20,-25.5,61,0.88,240,10,300.5,303.39999999999998,300.60000000000002,-25.561091040025751,-21.088420867919922]
[500,5450,-25.5,-29.5,69,0.67,315,6,301.89999999999998,304.2,302,-29.493755245701667,-26.093936920166016]
[432,6495,-33.700000000000003,-40.700000000000003,49,0.25,246,5,304.3,305.3,304.39999999999998,-40.684371156211704,-33.997444152832031]
[419,6708,-35.700000000000003,-41.7,54,0.24,232,4,304.39999999999998,305.3,304.5,-41.644777122091298,-35.862129211425781]
[412,6826,-36.5,-46.5,35,0.14000000000000001,224,4,304.89999999999998,305.39999999999998,304.89999999999998,-46.346329409357843,-36.452049255371094]
[400,7030,-38.5,-46.5,43,0.15,210,4,304.89999999999998,305.39999999999998,304.89999999999998,-46.337318454571054,-38.385593414306641]
[390,7203,-40.1,-47.1,47,0.14000000000000001,198,4,305,305.5,305,-47.029844194222143,-39.915611267089844]
[383,7326,-41.1,-51.1,33,0.09,190,4,305.3,305.60000000000002,305.3,-51.01269129369296,-40.555690765380859]
[376,7451,-42.1,-55.1,23,0.06,208,5,305.60000000000002,305.8,305.60000000000002,-54.901391934253041,-41.050018310546875]
[356,7814,-45.1,-57.3,24,0.05,260,10,306.3,306.5,306.3,-57.186986807812097,-43.771915435791016]
[339,8140,-47.8,-59.2,26,0.04,265,21,306.89999999999998,307.10000000000002,306.89999999999998,-58.939887152287774,-46.311550140380859]
[330,8319,-49.3,-60.3,26,0.03,295,27,307.3,307.39999999999998,307.3,-60.269679571629382,-47.666679382324219]
[327,8378,-49.4,-62.5,20,0.03,305,29,307.89999999999998,308,307.89999999999998,-62.345958027998748,-47.327259063720703]
[311,8706,-50.1,-74.2,4,0.01,320,43,311.39999999999998,311.39999999999998,311.39999999999998,-74.158034160777078,-44.77557373046875]
[307,8790,-50.3,-77.3,3,0,318,43,312.3,312.3,312.3,-76.159795957886672,-44.316780090332031]
[300,8940,-51.3,-70.3,9,0.01,315,43,312.89999999999998,313,312.89999999999998,-69.672444958870003,-47.529056549072266]

{"sheet":"DP+WB","index":4,"n_rows":27,"n_cols":4,"rows_kept":27,"cut":false,"hidden":false,"merged":[[0,0,0,2],[11,0,11,2],[20,0,20,2]]}
["Dew Point & Wet Bulb Calculation"]
[]
["Temperature",-51.3,"[°C]"]
["Relative Humidity",9,"[%]"]
["Absolute Pressure",300,"[hPa]","(this is not the pressure at sea level)"]
[]
[]
["Dew Point",{"$f":"B19*B14/(B13*LN(10)-B19)","v":-69.672444958870003},"[°C]"]
["Wet Bulb",{"$f":"(B27-32)*5/9","v":-47.529056236933052},"[°C]"]
[]
[]
["dew point"]
["Costante C",7.5]
["Costante K",237.7]
["Costante Z",6.11]
["Variabile D",{"$f":"(B13*B3)/(B14+B3)","v":-2.0641094420600861}]
["Variabile ES",{"$f":"B15*10^B16","v":5.2714703507473211E-2}]
["Variabile E",{"$f":"B4*B17/100","v":4.7443233156725887E-3}]
["Variabile D2",{"$f":"LN((B18/B15))","v":-7.1607332402476835}]
[]
["wet bulb"]
["Temperatura ",{"$f":"B3*9/5+32","v":-60.34},"[°F]"]
["Temperatura Dew Point",{"$f":"B8*9/5+32","v":-93.410400925966002},"[°F]"]
["Costante A",{"$f":"(B22-B23)/10","v":3.3070400925965999}]
["Costante B",{"$f":"B24-1","v":2.3070400925965999}]
["Costante D",{"$f":"B5/33.8639","v":8.8589914333552837}]
["Temperatura Bulbo Umido",{"$f":"B22-(0.034*B24-0.00072*B24*B25)*(B22+B23-2*B26+108)","v":-53.552301226479493},"[°F]"]